********************************************************************************************************************
The information in this ZIP file is confidential to Ross Video. 
If you are not the intended recipient, please notify me immediately by replying to the message which contained this. 
Please also delete all copies
********************************************************************************************************************

This file is for partner use when developing cards for the Ross Video OpenGear 3.0 frame.

This file was generated on March 11 2015.
It is a representation of:  8322AR-200-05 (this is an internal Ross number)

It represents: 
a) the (soon to be released ~mid 2015) full 20 position moulded card guide system 
b) the reinforced frame mounting brackets which are permanently attached to the chassis base part
c) newest version rear supports (bent sheet metal) used in frames after ~early 2014
d) older  version rear supports (cylindrical threaded rods) used in frames before ~early 2014 (this item is included as there are still many frames in the field which have these)

***************************************
***IMPORTANT TO THE PARTNER DESIGNER***
***************************************
1)	When designing new module concepts which don’t follow our standard MEC1 or HSEC8 rear module connectors as depicted in the OGx Dev Guide, Ross Mechanical Design should be consulted via your Ross Video contacts.
2)	The 3D should always be used in conjunction with the latest OGx Dev Guide and the card keepout specs it contains.
3)	Any discrepancies should be highlighted back to Ross Mechanical Design via your Ross Video contacts.
4)      Please direct any questions through to Ross Mechanical Design via your Ross Video contacts.

MJS